{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Data","Appendages-ed"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":100,"n_cols":11,"rows_kept":100,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["From-NODE - To-NODE","Diameter","Druktrap","Fitting / Beschrijving","Bemating","Eenheid","Link n Dir / File",null,null,null," = bekende maat uit tekening"]
[" 10-20","3\"","150#","Weldneck Flange",300,"mm","Map1.xlsm"]
[null,null,null,null,null,null,"Gewicht",null,null,null," = totaal maat van pijpdeel"]
[]
[]
[" 10-20","4\"","150#","Weldneck Flange",76,"mm",{"$f":"(7.37+1.56)*10","v":89.3},"N"]
[]
[null,null,null,"Elevatie +",10059]
[null,null,null,"Elevatie +",-9704]
[null,null,null,"Hoogte-Verschil",{"$f":"SUM(E11:E12)","v":355}]
[]
[null,null,null,null,7343]
[null,null,null,null,-1790]
[null,null,null,null,-1050]
[null,null,null,null,-1050]
[null,null,null,"MaatVerschil",{"$f":"SUM(E15:E18)","v":3453}]
[]
[null,null,null,null,557]
[null,null,null,null,4100]
[null,null,null,null,-3150]
[null,null,null,"MaatVerschil",{"$f":"SUM(E21:E23)","v":1507}]
[]
[null,null,null,"Elevatie +",7445]
[null,null,null,null,-550]
[null,null,null,"Elevatie +",{"$f":"SUM(E26:E27)","v":6895}]
[]
[null,null,null,"Elevatie +",12966]
[null,null,null,null,-9704]
[null,null,null,null,{"$f":"SUM(E30:E31)","v":3262}]
[]
[null,null,null,"Elevatie +",12966]
[null,null,null,null,-6895]
[null,null,null,null,{"$f":"SUM(E34:E35)","v":6071}]
[]
[null,null,null,null,7500]
[null,null,null,null,-3150]
[null,null,null,null,-1507]
[null,null,null,null,{"$f":"SUM(E38:E40)","v":2843}]
[]
[]
[null,null,null,null,{"$f":"E41","v":2843}]
[null,"3\"","150#","BW Equal Tee",-105,"mm"]
[null,null,null,"BW Conc. Reducer",-102,"mm"]
[null,null,null,null,{"$f":"SUM(E44:E46)","v":2636}]
[]
[null,null,null,null,1257]
[null,null,null,null,243]
[null,null,null,null,{"$f":"SUM(E49:E50)","v":1500}]
[]
[null,null,null,null,1650]
[null,null,null,null,-525]
[null,null,null,null,{"$f":"SUM(E53:E54)","v":1125}]
[]
[null,null,null,null,{"$f":"E55","v":1125}]
[null,"3\"","150#","Weldneck Flange",-70,"mm",{"$f":"(5.27+0.78)*10","v":60.5},"N"]
[null,null,null,null,{"$f":"SUM(E57:E58)","v":1055}]
[]
[null,null,null,null,525]
[null,"3\"","150#","Weldneck Flange",-70,"mm",{"$f":"(5.27+0.78)*10","v":60.5},"N"]
[null,null,null,null,{"$f":"SUM(E61:E62)","v":455}]
[]
[null,null,null,null,900]
[null,"3\"",null,"BW Equal Tee",-86]
[null,"3\" x 2\"",null,"BW Conc. Reducer",-89]
[null,"2\"","150#","Weldneck Flange",-64,"mm",{"$f":"(2.8+0.76)*10","v":35.599999999999994},"N"]
[null,"2\"","150#","Ball valve",-178,null,{"$f":"(14.66*10)","v":146.6},"N"]
[null,"2\"","150#","Weldneck Flange",-64,"mm",{"$f":"(5.27+0.78)*10","v":60.5},"N"]
[null,"2\"","150#","BW 90° LR Elbow",-76,"mm"]
[null,null,null,null,{"$f":"SUM(E65:E71)","v":343}]
[]
[]
[null,null,null,"Elevatie +",8245]
[null,null,null,"Elevatie +",-7445]
[null,null,null,"Hoogte-Verschil",{"$f":"SUM(E75:E76)","v":800}]
[]
[null,null,null,null,150]
[null,"2\"","150#","Weldneck Flange",-64,"mm",{"$f":"(2.8+0.76)*10","v":35.599999999999994},"N"]
[null,null,null,null,{"$f":"SUM(E79:E80)","v":86}]
[]
["900#",1333,"mm",null,{"$f":"E77","v":800}]
[null,null,null,null,-86]
[null,"2\"","150#","Weldneck Flange",-64,"mm",{"$f":"(5.27+0.78)*10","v":60.5},"N"]
[null,"2\"","150#","Weldneck Flange",-64,"mm",{"$f":"(5.27+0.78)*10","v":60.5},"N"]
[null,"2\"","150#","BW 90° LR Elbow",-76,"mm"]
[null,null,null,null,{"$f":"SUM(E83:E87)","v":510}]
[]
[null,null,null,null,1507]
[null,null,null,"BW Equal Tee",-105]
[null,null,null,"BW Conc. Reducer",-102]
[null,null,null,null,{"$f":"SUM(E90:E92)","v":1300}]
[]
[null,null,null,null,1093]
[null,null,null,null,1500]
[null,null,null,null,{"$f":"SUM(E95:E96)","v":2593}]
[]
[]
[null,null,"BW 180° SR Return","3\"",234,"mm"]

{"sheet":"Appendages-ed","index":1,"n_rows":47,"n_cols":13,"rows_kept":47,"cut":false,"hidden":false,"merged":[]}
["FromNode-ToNode"," 10-20","1/4\"","1/2\" x 3/4\"","150#","Weldneck Flange","BW 45° Elbow","SW 45° Elbow","Pipe Lengte","Control Valve","Strainer","DN10","DN10 x DN15"]
["Diameter"," 20-30","1/2\"","1\" x  3/4\"","300#","Slip-on Flange","BW 90° LR Elbow","SW 90° LR Elbow","Pipe Lengte IN SW flange","Safety Valve","Check Valve","DN15"]
["Reducers"," 30-40","3/4\"","1\" x 1/2\"","600#","Blind Flange","BW 180° LR Return","SW 180° LR Return","Min Speling","Flowmeter","Gate Valve","DN20"]
["ANSI Druktrappen"," 40-50","1\"","1 1/4\" x 1/2\"","900#","Threaded Flange","BW 90° SR Elbow","SW 90° SR Elbow","Max Speling","Massameter","Globe Valve","DN32"]
["Flange Type"," 50-60","1 1/2\"","1 1/4\" x 3/4\"","1500#","SocketWelded Flange","BW 180° SR Return","SW 180° SR Return","Vrije Ruimte"," -","Butterfly Valve","DN40"]
["Fittings BW"," 60-70","1 3/4\"","1 1/4\" x 1\"","2500#","Lapped Flange","BW Equal Tee","SW Equal Tee","Vrije Ruimte tot Vloer",null," -","DN50"]
["Omschrijving"," 70-80","2\"","1 1/2\" x 1/2\"","3000#","Long Welding Neck Flange","BW Reducing Tee","SW Reducing Tee","Vrije Ruimte tot Obstakel",null,null,"DN65"]
["Instrumenten"," 80-90","2 1/2\"","1 1/2\" x 3/4\"","6000#"," -","BW Cap","SW Cap","Hoogte Support",null,null,"DN80"]
["Appendages"," 90-100","3\"","1 1/2\" x 1\"","800#",null,"BW Conc. Reducer","SW Conc. Reducer","Elevatie +",null,null,"DN100"]
[null," -","4\"","1 1/2\" x 1 1/4\""," -",null,"BW Ecc. Reducer","SW Ecc. Reducer","Hoogte-Verschil",null,null,"DN125"]
[null,null,"5\"","2\" x 3/4\"",null,null,"BW Lap Joint Stub End","SW Lap Joint Stub End","MaatVerschil",null,null,"DN150"]
[null,null,"6\"","2\" x 1\"",null,null," -"," -"," -",null,null,"DN200"]
[null,null,"8\"","2\" x 1 1/4\"",null,null,null,null,null,null,null,"DN250"]
[null,null,"10\"","2\" x 1 1/2\"",null,null,null,null,null,null,null,"DN300"]
[null,null,"12\"","2 1/2\" x 1\"",null,null,null,null,null,null,null,"DN350"]
[null,null,"14\"","2 1/2\" x 1 1/4\"",null,null,null,null,null,null,null,"DN400"]
[null,null,"16\"","2 1/2\" x 1 1/2\""]
[null,null,"20\"","2 1/2\" x 2\""]
[null,null," -","3\" x 1`1/4\""]
[null,null,null,"3\" x 1`1/2\""]
[null,null,null,"3\" x 2\""]
[null,null,null,"3\" x 2`1/2\""]
[null,null,null,"3 1/2\" x 1 1/4\""]
[null,null,null,"3 1/2\" x 1 1/2\""]
[null,null,null,"3 1/2\" x 2\""]
[null,null,null,"3 1/2\" x 2 1/2\""]
[null,null,null,"3 1/2\" x 3\""]
[null,null,null,"4\" x 1 1/2\""]
[null,null,null,"4\" x 2\""]
[null,null,null,"4\" x 2 1/2\""]
[null,null,null,"4\" x 3\""]
[null,null,null,"4\" x 3 1/2\""]
[null,null,null,"5\" x 2\""]
[null,null,null,"5\" x 2 1/2\""]
[null,null,null,"5\" x 3\""]
[null,null,null,"5\" x 3 1/2\""]
[null,null,null,"5\" x 4\""]
[null,null,null,"6\" x 2 1/2\""]
[null,null,null,"6\" x 3\""]
[null,null,null,"6\" x 3 1/2\""]
[null,null,null,"6\" x 4\""]
[null,null,null,"6\" x 5\""]
[null,null,null,"8\" x 3 1/2\""]
[null,null,null,"8\" x 4\""]
[null,null,null,"8\" x 5\""]
[null,null,null,"8\" x 6\""]
[null,null,null," -"]